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To be read with Preliminaries/General conditions

160/01
DUCT LININGS – PREPLUMBED PANELS AND PROPRIETARY FRAMES
Drawing reference(s):  
· Manufacturer and reference: Venesta Washroom Systems, Unit 19-23, St George’s Shopping Centre, Gravesend, Kent, DA11 0TA
· Product: Hygen PVC Box Unit.
· Panel: Joint free 15mm closed cell PVC board faced with 2.5mm PVC sheet with postformed corners and 2 hinged recessed access panels, complete with locks and seal.
· Panel thickness: 17.5mm.
· Panel/finish: Colour/finish: 11 standard colours, 24 premium colours - a choice of satin or gloss finishes.
· Access: Rebated or overlapping door.

· Hinge: 160 degree overlay hinge secured to bespoke zinc plated steel bracket.  
· Panel seal: Access panels incorporating a 3mm self adhesive C211 FR flame retardant neoprene sponge seal.
· Lock: Manufactured from stainless steel with a polished finish, with master key.
· Box unit secured using Venesta tie back system incorporating M8 zinc plated tie-back rods and supporting bracketry in zinc plated steel.

· Height: Up to maximum box height 3000mm to suit a fixed ceiling or 2940mm to suit a suspended ceiling.

· Width: 700mm to 800mm depending on depth/arrangement.
· Depth: 150mm and 225mm depth as standard. 

· Pre-plumbing: Sanitary appliances as specified in section N13, pre-fixed and sealed to HBN box out unit, unless stated otherwise, all factory assembled.
· Options: Colour matched silicone and weld rod available.
